[config]
line_0_com = COM9
agbaud=921600

filter_embedusb=1
filter_externcom=0
filter_explicitcom0 = 19D1
filter_explicitcom1 = 1366
;agentboot.bin file infomation
[agentboot]
tool_basedir = 1
agpath =.\image_ec626\agentboot.bin

[storage_cfg]
opt_storage_list=""
format_path=format_ec626.json

;bootloader.bin file infomation
[bootloader]
blpath = .\image_ec626\bootloader.bin

blloadskip = 0

;system.bin file infomation
[system]
syspath =.\image_ec626\ap_demo-flash.bin
sysloadskip = 0
burnaddr = 0x1f000

;control such as reset before download
[control]
detect = 2
atbaud=115200

prempt_detect_time = 6
msg_waittime = 2
max_preamble_cnt = 8
lpc_recover_en = 0
;cfg reset to 2, skip reset pin
pullup_qspi =1
;remap_dld_addr = 32768
rom_version=0000000104000000
;send and receive


[flexfile0]
filepath = .\rfCaliTb_ec626\MergeRfTable_flx0_chocie_0.bin
burnaddr = 0x1dc000
storage_type=ap_flash

;add support for choice flexfile by chipid
choose_path_by_chipid=1
;select_chipid_mode =file_chipid_by_ordered_index 
select_chipid_mode=file_chipid_by_compare_seq

;(CHIP ID0)
index0_chipid=a0efe8ee
index0_compseq=0x0:36

;(CHIP ID1)
index1_chipid=b08690f0
index1_compseq=0x0:37

flxchoc_allow_getattr_dbg=1

[flexfile1]
filepath = .\rfCaliTb_ec626\MergeRfTable_flx1_chocie_0.bin
burnaddr = 0x15000
storage_type=ap_flash

;add support for choice flexfile by chipid
choose_path_by_chipid=1
;select_chipid_mode =file_chipid_by_ordered_index 
select_chipid_mode=file_chipid_by_compare_seq

;(CHIP ID0)
index0_chipid=a0efe8ee
index0_compseq=0x0:36

;(CHIP ID1)
index1_chipid=b08690f0
index1_compseq=0x0:37

flxchoc_allow_getattr_dbg=1
